62,G:\资料\2_RW合封资料\可提供给客户的合封资料\RW1602H\1602H_V1.0\01_例程\rw1602h_rls_v1.1\sysmain.c	Line 62	: [Warning] use time : -0.032000 Sec (-32 msec)
180,G:\资料\2_RW合封资料\可提供给客户的合封资料\RW1602H\1602H_V1.0\01_例程\rw1602h_rls_v1.1\CarApp.c	Line 180	: [Warning] use time : -0.020000 Sec (-20 msec)
142,G:\资料\2_RW合封资料\可提供给客户的合封资料\RW1602H\1602H_V1.0\01_例程\rw1602h_rls_v1.1\CarApp.c	Line 142	: Warning #5: User [Warning] P.0
483,G:\资料\2_RW合封资料\可提供给客户的合封资料\RW1602H\1602H_V1.0\01_例程\rw1602h_rls_v1.1\rw1620drv.c	Line 483	: [Warning] `temp00' is defined but never used
483,G:\资料\2_RW合封资料\可提供给客户的合封资料\RW1602H\1602H_V1.0\01_例程\rw1602h_rls_v1.1\rw1620drv.c	Line 483	: [Warning] `tmp_data' is defined but never used
585,G:\资料\2_RW合封资料\可提供给客户的合封资料\RW1602H\1602H_V1.0\01_例程\rw1602h_rls_v1.1\rw1620drv.c	Line 585	: [Warning] use time : 0.040000 Sec (40 msec)
135,G:\资料\2_RW合封资料\可提供给客户的合封资料\RW1602H\1602H_V1.0\01_例程\rw1602h_rls_v1.1\timer.c	Line 135	: [Warning] use time : -0.029000 Sec (-29 msec)
0,LINK: [Warning] <<< ORG define address 0095h be shift to 0096h in file the file>>>
0,LINK: [Warning] <<< ORG define address 0095h be shift to 0097h in file the file>>>
0,LINK: [Warning] <<< ORG define address 0095h be shift to 0096h in file the file>>>
0,LINK: [Warning] <<< ORG define address 0095h be shift to 0097h in file the file>>>
-1,[Message]LINK: Call Tree (Max Deep): _rf_recive_data_test(1):_rf_RecivePack(2):_init_rf(3):_rf_bank_Switch(4):_get_rf_status_flag(5):_spi_Writeabyte(6)
-1,[Message]LINK: start address of RAM variable is 0x20
-1,Program Memory Usage (Used=1225, Unused=823)